**The specs below are for the ranges.**

Here are the links they are pulled from:

30” - <https://kucht.com/online/product/model-kng301-color-series/>

36” - <https://kucht.com/online/product/model-kng361-color/>

48” - <https://kucht.com/online/product/model-kng481-color-series/>

**BOLD/Classico Specs**

48" BOLD and Classico

PERFORMANCE

8 BURNERS & Removable Professional Griddle / Grill

2 x 20,000 BTU dual burner with simmer

2 x 12,000 BTU burner

2 x 9,000 BTU burners

2 x 6,000 BTU burner

MAIN OVEN

4.2 Cu. Ft. Oven
 22,000 BTU Convection Oven (Gas version)
 10,000 BTU Broiler (Gas Version)

SECONDARY OVEN

2.5 Cu. Ft. Oven Capacity
 10,000 BTU Tube Burner (Gas Version)

DESIGN

Removable Professional Griddle / Grill

Black porcelain top
 Blue porcelain oven interior
 Premium Quality Metal Control Knobs
 Extra Large Oven Window
 Heavy Duty Cast-Iron Cooking Grates
 4” Stainless Steel Backsplash
 Full Stainless Steel Side Panels
 Professional Handle

DETAILS

2 halogen lights oven interior
 2 layers glass window
 2 Oven Racks
 Fully Adjustable Heavy-duty Legs
 Manual Oven Control
 Electronic Ignition with Auto Re-ignition
 Manual Convection Cooking Mode
 4 years warranty for parts and labor

ACCESSORIES

– [Color Door and Kickplate](https://kucht.com/online/product/color-doors-kp-for-kng481-6-colors/)

– [Color Knobs](https://kucht.com/online/product/kng-color-knobs/)

[– Color Knob Rings / Bezels](https://kucht.com/online/product/kng-color-knob-rings-bezels/)

– Color Handle

– [Wok Stand](https://kucht.com/online/product/wok-stand/) (not included)

– [Grill/Griddle](https://kucht.com/online/product/grill-griddle-for-kng-series/) (included!)

– Natural Gas or Liquid Propane

DIMENSIONS

Overall Height: 36″ (40″ with backsplash)
 Overall Width: 48″
 Overall Depth: 28-7/8″

Electrical Requirements

120V/60Hz/15 or 20A (Gas Version)

NOTES

* The oven-knob displayed temperature is set to match the oven temperature with the convection mode on. When using the oven with the convection feature off, the temperature inside the oven could be between 25 to 50 degrees lower than the knob indicates.
* Due to the high power of the top burners, we do not recommend the use of downdraft ventilation systems. A range hood with at least 450 CFM is advisable.

**36” BOLD/Classico Specs**

**PERFORMANCE**

**6 BURNERS**

1 x 20,000 BTU dual burner with simmer
 1 x 15,000 BTU burner
 1 x 12,000 BTU burner
 2 x 9,000 BTU burners
 1 x 6,000 BTU burner

**OVEN**

5.2 Cu. Ft. Oven
 22,000 BTU Convection Oven (Gas Version)
 10,000 BTU Tube Burner Broiler (Gas Version)

**DESIGN**

Black porcelain top
 Blue porcelain oven interior
 Premium Quality Metal Control Knobs
 Extra Large Oven Window
 Heavy Duty Cast-Iron Cooking Grates
 4” Stainless Steel Backsplash
 Full Stainless Steel Side Panels
 Professional Handle

**DETAILS**

2 halogen lights oven interior
 2 layers glass window
 2 Oven Racks
 Fully Adjustable Heavy-duty Legs
 Manual Oven Control
 Electronic Ignition with Auto Re-ignition
 Manual Convection Cooking Mode
 4 years warranty for parts and labor

**ACCESSORIES**

– [Color Door and Kickplate](https://kucht.com/online/product/color-door-kickplate-for-kng361/)

– [Color Knobs](https://kucht.com/online/product/kng-color-knobs/)

[– Color Knob Rings / Bezels](https://kucht.com/online/product/kng-color-knob-rings-bezels/)

– Color Handle

– [Wok Stand](https://kucht.com/online/product/wok-stand/) (not included)

– [Grill/Griddle](https://kucht.com/online/product/grill-griddle-for-kng-series/) (included!)

– Natural Gas or Liquid Propane

**DIMENSIONS**

Overall Height: 36″ (40″ with backsplash)
 Overall Width: 36″
 Overall Depth: 28-7/8″

**Electrical Requirements**

120V/60Hz/15 or 20A (All-Gas Version)

**NOTES**

* The oven-knob displayed temperature is set to match the oven temperature with the convection mode on. When using the oven with the convection feature off, the temperature inside the oven could be between 25 to 50 degrees lower than the knob indicates.
* Due to the high power of the top burners, we do not recommend the use of downdraft ventilation systems. A range hood with at least 450 CFM is advisable.

**30” BOLD/Classico Specs**

**PERFORMANCE**

**4 BURNERS**

2 x 15,000 BTU burner
 2 x 9,000 BTU burners

**OVEN**

4.2 Cu. Ft. Oven
 22,000 BTU Convection Oven (Gas Version)
 10,000 BTU Tube Burner Broiler )Gas Version)

**DESIGN**

Black porcelain top
 Blue porcelain oven interior
 Premium Quality Metal Control Knobs
 Extra Large Oven Window
 Heavy Duty Cast-Iron Cooking Grates
 4” Stainless Steel Backsplash
 Full Stainless Steel Side Panels
 Professional Handle

**DETAILS**

2 halogen lights oven interior
 2 layers glass window
 2 Oven Racks
 Fully Adjustable Heavy-duty Legs
 Manual Oven Control
 Electronic Ignition with Auto Re-ignition
 Manual Convection Cooking Mode
 4 years warranty for parts and labor

**ACCESSORIES**

– [Color Door and Kickplate](https://kucht.com/online/product/color-door-kp-for-kng301-6-colors/)

– [Color Knobs](https://kucht.com/online/product/kng-color-knobs/)

[– Color Knob Rings / Bezels](https://kucht.com/online/product/kng-color-knob-rings-bezels/)

– [Color Handle](https://kucht.com/online/product/kng-color-knob-rings-bezels-2/)

– [Wok Stand](https://kucht.com/online/product/wok-stand/) (not included)

– Natural Gas or Liquid Propane

**DIMENSIONS**

Overall Height: 36″ (40″ with backsplash)
 Overall Width: 30″
 Overall Depth: 28-7/8″

**Electrical Requirements**

120V/60Hz/15 or 20A (Gas Version)

**NOTES**

* The oven-knob displayed temperature is set to match the oven temperature with the convection mode on. When using the oven with the convection feature off, the temperature inside the oven could be between 25 to 50 degrees lower than the knob indicates.
* Due to the high power of the top burners, we do not recommend the use of downdraft ventilation systems. A range hood with at least 450 CFM is advisable.